1. Close the program access to the Internet in hosts or otherwise to:
    activate.electronic.us
    appstatico.electronic.us
    cdn.electronic.us
2. Install usb_network_gate.exe v10.0.2450.0 (other versions are not supported by the patcher).
3. Run patcher.exe with admin rights, wait for the process to complete.
4. Run the program and activate manually:
    a) enter the key 12345-12345-12345-12345-12345 (or any other from the character set [0-9][A-F])
    b) select manual mode
    c) save the request file UNG-activation-info.activate , do not close the manual activation window.
    d) create an activation file UNG-activation-info.bin by dropping the file UNG-activation-info.activate on activator.exe
    e) load UNG-activation-info.bin from the manual activation window, wait for the process to complete.